|  |  |
| --- | --- |
| Lock Out Tag Out | Unit: Extruder |
| Date Created: 4/17/23 | Last Reviewed: 4/17/23 |

1. A picture containing text, indoor, several

   Description automatically generatedPress the Emergency Stop Button down.
2. A picture containing disk brake, helmet

   Description automatically generatedUnplug the power from the wall. The plug is marked with yellow tape. Place lock around the plug.

LOTO #1